

JSS MAHAVIDYAPEETHA

**SJCE – Science & Technology Entrepreneurs Park, Mysuru   
 (SJCE-STEP)** (A Society registered under Societies Registration Act 1960)

Supported by the Dept. of Science & Technology, Govt. Of India

JSS Technical Institutions Campus, Mysuru – 570006, Karnataka, India, Ph. No.- 0821 2548321

# SJCE-STEP : NIDHI PRAYAS

**SHORT TERM TENDER DOCUMENT**

# For “*Supply, Installation and maintenance of Machineries”*

Tender Reference Number: SJCE-STEP/NIDHI PRAYAS/2022-23/01

Date: 02.02.2023

Tender documents can be downloaded from the website <https://eproc.karnataka.gov.in>

**Sri Jayachamarajendra College of Engineering - Science & Technology Entrepreneurs Park (SJCE-STEP),**

**JSS Technical Initiation Campus, Manasagangotri**

**MYSURU – 570006.**

Phone: 0821-2548321  
e-mail: info@sjcestep.in | website: http://www.sjcestep.in

# Request for Quotation

SJCE-STEP, invites offers through e-procurement from eligible reputed OEM’s or their authorized dealers/ vendors hereinafter called as ‘vendor/ bidder’ for Supply, Installation and maintenance of Machineries to Sri Jayachamarajendra College of Engineering - Science & Technology Entrepreneurs Park (SJCE-STEP), JSS TI CAMPUS, MYSURU – 570006.

The details are given below:

|  |  |
| --- | --- |
| Tender Reference | SJCE-STEP/NIDHI PRAYAS/2022-23/01 |
| EMD | 2.5% on each equipment. |
| Tender Publishing date | 02.02.2023 |
| Last Date for receipts of offer | 21.02.2023 - 17:00 Hours |
| Date and time of opening of offer | 23.02.2023 - 11:00 Hours |
| Opening of financial bid | 27.02.2023 |
| Address for Communication | The Chief Executive  Sri Jayachamarajendra College of  Engineering - Science & Technology  Entrepreneurs Park  JSS Technical Institutions Campus,  Mysuru – 570006, Karnataka, India |
| Contact Telephone Numbers | 0821-2548321 |

**1. About the SJCE-STEP;**

Sri Jayachamarajendra College of Engineering - Science & Technology Entrepreneurs Park is a Technology Business Incubator with the objective of supporting startup entrepreneurs.

**2. Objective and scope of this Tender**

Supply, Installation and maintenance of *Machineries.*

**3. Qualification Criteria**

Only the vendor/ bidder who meets all the qualifications mentioned in **Annexure-1 “Qualification Criteria”** of the tender are eligible to participate in the tender.

**4. Terms and Conditions**

The Terms and conditions for vendor/ bidder who participates in this tender are specified in **Annexure-2 “Terms and Conditions”**. These terms and conditions are binding on all the vendor/ bidder. These terms and conditions will also form part of the purchase order, to be issued to the successful vendor/ bidder on the outcome of the tender process.

**5. Earnest Money Deposit (EMD)**

Vendor/ bidder are required to deposit EMD of Rs. 1,00,000/- (Rupees one Lakh only) shall pay through e-procurement following modes

**Online Payments:**

*i. Credit card*

*ii. Debit card*

*iii. Net banking*

Offers made without E.M.D. will be summarily rejected. No interest would be payable on the EMD amount. The EMD shall be refundable to un-successful bidders after placing Purchase Order to the successful bidder. EMD of the successful tenderer will be refunded after the receipt of Performance Bank Guarantee.

**6. Forfeiture of EMD**

If the successful vendor/ bidder fails to fulfill the obligations specified in this tender document, EMD paid by the successful vendor/ bidder will be forfeited.

**7. Offer Validity Period**

The offer should be valid for a period of 90 days from the date of the opening of financial bid of the tender.

**8. Address for Communication**

The Chief Executive

Sri Jayachamarajendra College of Engineering - Science

& Technology Entrepreneurs Park

JSS Technical Institutions Campus, Mysuru – 570006,

Karnataka, India

**9. Proposal Ownership**

The proposal and all supporting documents submitted by the vendor/ bidder in this tender process shall become the property of the SJCE-STEP.

**10. Modification and Withdrawal of Offers**

Vendor/ bidder are not allowed to modify their offer once submitted. No offer can be withdrawn by a vendor/ bidder after the closing date and time for submission of offers.

**11. Opening of offers**

Vendors who qualify in the technical bid shall only be called during the opening of the financial bid. The vendor/ bidder present shall sign a register of attendance.

**12. Preliminary Scrutiny**

Offers from vendor/ bidder not meeting the qualification criteria will be rejected. The Committee of the SJCE-STEP will scrutinize the offers received to determine whether they are complete and as per tender requirements, whether documentation as asked for and required to evaluate the offer has been submitted, whether the documents have been properly signed and whether items are offered as per the tender requirements.

**13. Clarification of Offers**

To assist in the scrutiny, evaluation and comparison of offers, the SJCE-STEP may, at its discretion, ask some or all vendor/ bidder for clarifications on the offer made by them in writing or by email. The request for such clarifications and the vendor/ bidder’s response will necessarily be in writing or email.

**14. No Commitment to Accept any Offer**

The SJCE-STEP shall be under no obligation to accept any offer received in response to this tender and reserves its right to reject all offers including complete offers without assigning any reason whatsoever. The SJCE-STEP reserves the right to make any changes in the terms & conditions of purchase as and when need is felt.

The SJCE-STEP will not be obliged to meet and have discussions with any vendor/ bidder and /or to entertain any representations which are deemed unfit.

**15. Documentation**

Technical information in the form of Brochures/ Manuals/ CD etc. must be submitted in support of the offer made.

**16. Submission of Technical Details**

It is mandatory to provide the technical details in the format of Technical Details & Specifications (**Annexure-3)**.

The offer may not be evaluated /may be rejected by the SJCE-STEP in case of non-adherence to the format or partial submission of technical information as per the format given in the offer. The deviations in the technical details should be mentioned in the technical offer only [**Annexure-3**] and on the contrary specifying the deviations elsewhere in the offer is not acceptable and will not be considered.

The SJCE-STEP shall not allow/permit changes in the technical details after due date for submission of offers.

**17. Technical Documents required in online submission**

1. Earnest Money Deposit (EMD) paid details
2. Tender processing fee paid details
3. Documents required to be submitted as mentioned in the **Annexure -1**
4. Technical Details & Specifications as given in **Annexure-3**.
5. Covering letter as per **Annexure-4** and be in the letter head of the vendor company.
6. Details of the vendor, as per **Annexure-5**.
7. Letter of Authenticity as in **Annexure-6.**
8. Manufactures Authorization Form (**MAF) Annexure-7.**
9. OEM Warranty certificate.
10. Experience Details as in **Annexure-10**.
11. Any other documents.

**18. Commercial bid required in online submission**

Document required to be submitted online is **Annexure-9**

**19. Erasures or Alterations**

The Offers containing erasures or alterations will not be considered. There should be no hand-written material, corrections or alterations in the offer. Technical details must be completely filled in. Correct technical information of the product being offered must be filled in. Filling up of the information using terms such as “OK”, “accepted”, “noted”, “as given in brochure/manual” is not acceptable. The SJCE-STEP may treat such Offers as not adhering to the tender guidelines and as unacceptable.

**20. Fixed Price**

The offer shall be on a fixed price basis, inclusive of all taxes and levies. No price increase due to increases in tax, dollar price variation etc. will be permitted. However, any downward revision of tax, dollar price, the benefit of which has to be passed on to the SJCE-STEP.

**21. Guarantees**

The vendor/ bidder should guarantee that the items delivered to the SJCE-STEP are brand new, including all components.

**22. Letter of undertaking of Authenticity**

The vendor/ bidder should give an undertaking in the format given in **Annexure-6**.

**23. Negotiation**

It is absolutely essential for the vendor/ bidder to quote the lowest price at the time of making the offer in their own interest, as the SJCE-STEP will not enter into any price negotiations, except with the lowest quoting vendor/ bidder (L1), in case of absolute necessity.

**24. Liabilities of SJCE-STEP**

This tender is not an offer by the SJCE-STEP, but an invitation for vendor/ bidder responses. No contractual obligation on behalf of the SJCE-STEP, whatsoever, shall arise from the tender process unless and until a formal work order is issued by duly authorized officer of the SJCE-STEP to the successful tenderer.

**25. Proposal Process Management**

The SJCE-STEP reserves the right to accept or reject any/all proposal/ to revise the tender document, to request one or more re-submissions or clarifications from one or more Vendor/ bidder, or to cancel the process in part or whole. No Vendor/ bidder are obligated to respond to or to continue to respond to the tender. Additionally, the SJCE-STEP reserves the right to alter the requirements, in part or whole, during the tender process. Each party shall be entirely responsible for its own costs and expenses that are incurred while participating in the tender, subsequent presentation and contract negotiation processes.

**26. Downloading of Tender document from following website:**

e-procurement website **https://eproc.karnataka.gov.in/**

But, it should be strictly noted here that the documents should be uploaded to the e-Procurement websiteonly. In case of any dispute/discrepancy the physical version of the tender available with the SJCE-STEP will be final & binding on all who participate in the tender.

**Annexure-1**

**QUALIFICATION CRITERIA**

1. The vendor/ bidder must have an office in Karnataka. Vendor/ bidder **should enclose attested copies of Property tax bill/ Lease agreement, Electricity Bill, Telephone Bill, GST Registration and PAN**.

2. The vendor/ bidder company/ firm should have an annual turnover of Rs 50lakhs or above from businesses relating to sales and support of Machineries in India during the last 3 years (2019-20, 2020-21, & 2021-22). **Vendor/ bidder should furnish copies of audited balance sheets for the last three years (2019-20, 2020-21, & 2021-22)** **in support of annual turnover or Certificates issued by Chartered Accountant.**

3. The vendor/ bidder should have experience for Supply, Installation and maintenance of Machineries. The bidder must have at least 5 customer reference sites installation in Karnataka. (**Annexure- 10).**

4. The vendor/ bidder should have an MAF for Supply, Installation and maintenance of Machineries from well reputed manufacturer. **Copy of the same need to be submitted.**

5. The OEM should have Service Center operating, Karnataka. Communication address and telephone number should be provided. **Copy of the document need to be submitted.**

**Annexure-2**

**TERMS AND CONDITIONS**

1. Quotes submitted must be clearly legible, duly signed by authorized signatories.
2. Time Schedule

* Indicating delivery, installation and commissioning.

1. Supply, Installation and maintenance of Machineries.
2. Bid Pricing and process:

* Prices shall be quoted in Indian Rupees only.
* Price shall be inclusive of all freight, forwarding, transit insurance and installation charges.
* Prices stated in the bid-offers submitted by vendor/ bidder/ OEM’s are in accordance with the tender document. The Vendor/ bidder further understand that the quantities and scope of work as specified in this tender may vary at the time of award of work order as per the discretion and requirements of SJCE-STEP.

1. Payment terms:

* No advance payment will be made.
* 90% of cost for the items supplied and on successful implementation as certified by SJCE-STEP.
* Balance 10% will be made after 45-60 days of satisfactory installation, acceptance by SJCE-STEP and on submission of Performance Bank Guarantee.

1. Taxes/Duties/Etc.: Prices shall be inclusive of taxes/ duties. The prices shall strictly be submitted in the given format. Quoted prices shall be indicated with the tax components as applicable and shall be mentioned separately in the respective columns.
2. Penalty:
   * Failure to supply and installation of Machineries within the time schedule as mentioned in Terms and Conditions above shall entail a penalty equal to 2% of the value of the bid price or forfeiture of EMD.
   * During the warranty period, if the complaint is not attended to within 48 hrs, penalty of Rs. 500 per day will be levied. The amount of penalty will be recovered from the Performance bank guarantee or the Performance Bank Guarantee will be forfeited.
3. Performance Bank Guarantee: Once the work order is raised and on the successful Supply, Installation, and maintenance of SJCE-STEP but before putting a request for the release of the balance 50% payment, the vendor/ bidder shall submit to the SJCE-STEP a Performance Bank Guarantee as in Annexure -8 (PBG) worth 50% of the cost of the Work Order value, valid for the entire warranty period.
4. The Goods must be Delivered within 30 days or earlier form the date of P.O
5. WARRANTY:

* Onsite warranty shall be for a minimum period of (3) three years from the date of supply/ installation.
* In case, a part thereof or the whole equipment is found defective the same will have to be rectified/replaced on free of charge basis without lapse of time.
* If any equipment gives continuous trouble, say 3 times in one month during the warranty period, the bidder shall replace the equipment with new one without any additional cost to SJCE-STEP.

1. The location where the Machineries is to be installed shall be identified and finalized in consultation with the SJCE-STEP.
2. Resolution of Disputes: Machineries and the vendor/ bidder shall make every effort to resolve issues amicably, by direct informal negotiation, any disagreement or dispute arising between them under or in connection with the contract. If after 30 (thirty) days from the commencement of such informal negotiations, the SJCE-STEP and the Vendor/ bidder are unable to resolve amicably a contract dispute; either party may require that the dispute be referred for resolution by formal arbitration.
3. All questions, disputes, or differences arising under and out of, or in connection with the contract, shall be referred to two Arbitrators: one Arbitrator to be nominated by the SJCE-STEP and the other to be nominated by the Vendor/ bidder. In the case of the said Arbitrators not agreeing, then the matter will be referred to an umpire to be appointed by the Arbitrators in writing before proceeding with the reference. The award of the Arbitrators, and in the event of their not agreeing, the award of the Umpire appointed by them shall be final and binding on the parties. The Arbitration and Reconciliation Act 1996 shall apply to the arbitration proceedings and the venue of the arbitration shall be Mysuru.

Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (name)

on behalf of

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Name of the vendor/ bidder)

**Annexure-3**

Minimum Technical Specifications for Machineries

Bill of quantity per unit:

|  |  |  |
| --- | --- | --- |
| **SI No.** | **Items** | **Specification** |
| 1 | 3D Scanner | Maker: Artec or Equivalent  Details: Hand Held Device  Technical specifications:   * Scanner type: handheld * 3D point accuracy,Up to 0.1 mm * 3D resolution,upto 0.5 mm * 3D accuracy over distance, upto 0.1mm+0.3mm/m |
| 2 | CNC - Router | Maker: Stepcraft or Equivalent  Details: CNC Router (With MultiHeads & Ball Probe)  Technical specifications:   * Machine's Footprint (Width, Length, Height) : 36" x 48.3" x 25.4" * X-Travel : 679 mm * Y-Travel : 1044 mm * Z-Travel : 194 mm |
| 3 | 3D Printer - FDM | Maker: Divide by Zero or Equivalent  Details: Minimum Bed Size - 400\*300\*300  Technical specifications:   * Build Size: 400mm X 300mm X 300mm * NOZZLE Diameter: 0.4mm - 0.8mm (optional ) * Extruder: Single (upgradeable to dual) * Noise Level: <55 dB * Accuracy 80-250 Micron |
| 4 | Laser Cutting Machine | Maker: VM Technologies Or Equivalent  Details: 4 Feet X 3 Feet  Technical specifications:   * Laser Type : CO2 * Working Area: 4 Feet X 3 Feet * with all standard accessories |
| 5 | Laser Engraving Machine | Maker: [Yugma Impressions](https://www.copiainc.net/)  Details:  Technical specifications:   * Minimum line width: 0.01mm * Minimum character: 0.1mm * Marking speed: 0-7000m/s * Cooling system: air cooling * Repeat accuracy: 0.01mm * Input power: AC 220V 10% 50Hz (60Hz) * Lifetime: 100,000 hours (if properly operated) * Maintenance Free Laser Engine * Motorized or Manual Z-Adjustment * Easily Integrated Footprint |
| 6 | 3D Printer - SLA | Maker: [Prusa or Equivalent](https://www.copiainc.net/)  Technical specifications:   * LCD resolution 5.96'', 2560×1620p * LCD lifespan / warranty 2000 hours * Minimum Print volume size 127×80×150 mm * Layer exposure time 1.3 - 2.4 seconds depending on material and layer height * Tilt time 3 seconds * with all standard accessories |
| 7 | CNC wire EDM Cutting Machine | Maker: Fostex Or Equivalent  Technical specifications:  CNC-wire cut Electric discharge machine with single cut Control Cabinet (3 Phase, 45V/50Hz) and standard Accessories steel cover, LM Guide, High Pressure coolant pump & tool Box. |

**Annexure 4**

(Should be in the letterhead of the Company)

Offer Reference No.:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_2023

To:

The Chief Executive

SJCE-STEP, JSS Technical Initiation Campus,

Manasagangotri, Mysuru – 570006.

Dear Sir/Madam,

Tender Ref:

Having examined the tender document including all Annexures the receipt of which is hereby duly acknowledged, we, the undersigned, offer to “*Supply, Installation, and maintenance of Machineries*” in conformity with the said tender in accordance with the Schedule of Prices indicated in the offer and made part of this offer.

If our offer is accepted, we undertake to complete delivery & installation within the time frame mentioned in the terms and conditions.

We agree to abide by this offer till --- days from the date of opening of the commercial offer by the SJCE-STEP and our offer shall remain binding upon us and may be accepted by the SJE-STEP any time before the expiration of that period.

Until a formal contract is prepared and executed, this offer, together with the SJCE-STEP’s written acceptance thereof and the SJCE-STEP’s notification of award, shall constitute a binding contract between us.

We understand that the SJCE-STEP is not bound to accept the lowest or any offer the Corporation may receive without assigning any reason whatsoever.

We certify that we have not been blacklisted / barred to participate in Tender or to supply hardware by any of the Public Sector Under takings, Government Organizations and Public Sector Banks in India.

Dated this \_\_\_\_\_\_ day of \_\_\_\_\_\_\_\_\_2023

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(in the Capacity of:) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name:

Contact No:

Email id:

**Annexure 5**

**Details of the Vendor/ bidder**

Details filled in this form must be accompanied by sufficient documentary evidence, in order to facilitate the SJCE-STEP to verify the correctness of the information.

|  |  |  |
| --- | --- | --- |
| S.No | **Item** | **Details** |
| 1 | Name of Company/ firm |  |
| 2 | Postal Address |  |
| 3 | Telephone, mobile and Fax numbers |  |
| 4 | Constitution of the Company |  |
| 5 | Name and designation of the person authorized to make commitments to this tender |  |
| 6 | Bank Name |  |
| 7 | Account No |  |
| 8 | Branch Name |  |
| 9 | IFSC Code |  |
| 10 | MICR No. |  |
| 11 | Email Address |  |
| 12 | Year of commencement of Business |  |
| 13 | Sales Tax Registration Number |  |
| 14 | Income Tax PAN Number |  |
| 15 | GST number |  |
| 16 | Whether OEM or authorized dealer/agent |  |
| 17 | Name and Address of OEM |  |
| 18 | Website address of the Company |  |

Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (name)

on behalf of

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Name of the vendor/ bidder)

**Annexure 6**

LETTER OF UNDERTAKING OF AUTHENTICITY

1. We undertake that all the components/parts /software used in the Supply and Installation of Supply*, Installation and maintenance of Machineries* supplied shall be original, new components & software only and that no refurbished/duplicate/ second hand components/ parts/ assembly/ software are being used.

2. We hereby undertake to produce the certificate from an OEM in support of above undertaking at the time of delivery/ installation. It will be our responsibility to produce such letters from our OEM suppliers at the time of delivery or within a reasonable time.

Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (name)

on behalf of

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Name of the vendor/ bidder)

**Annexure 7**

**MANUFACTURERS' AUTHORIZATION FORM (MAF)**

No. Dated

To:

The Chief Executive

SJCE-STEP, JSS Technical Initiation Campus,

Manasagangotri, Mysuru – 570006.

Dear sir/Madam:

We \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_who are established and reputable manufacturers of having factories at\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (address of factory) do hereby authorize M/s.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (Name and address of Agent) to submit a bid, negotiate and receive the order from you.

No company or firm or individual other than M/s. \_\_\_\_\_\_\_\_\_\_\_\_ is authorized to bid, and conclude the contract in regard to this business.

We hereby extend our full guarantee and warranty as per the Tender Document SJCE-STEP/NIDHI PRAYAS/2022-23/01 of the Terms and Conditions for the goods and services offered by the above firm.

Yours faithfully,

(Name)

(Name of manufacturers)

**Note: This letter of authority should be on the letterhead of the manufacturer and should be signed by a person competent and having the power of attorney to bind the manufacturer. It should be included by the Bidder in its bid.**

**Annexure 8**

PERFORMANCE BANK GUARANTEE

(From scheduled Commercial Bank of India)

To:

The Chief Executive

SJCE-STEP, JSS Technical Initiation Campus,

Manasagangotri, Mysuru – 570006.

WHEREAS ............................(Company Name) registered under the Indian Companies Act 1956 and having its Registered Office at .............................................................., hereinafter referred to as the VENDOR/ BIDDER has undertaken to *Supply, Installation and maintenance of Machineries* to SJCE-STEP, Mysuru, Karnataka State, and demonstration of Guaranteed Performance in terms of the Purchase Order bearing No. .............. dated ......................, hereinafter referred to as “the CONTRACT.

AND WHEREAS in terms of the Conditions stipulated in the said Contract, the VENDOR/ BIDDER is required to furnish, performance Bank Guarantee issued by a Scheduled Commercial Bank in your favour to secure due and satisfactory compliance of the obligations of the VENDOR/ BIDDER in accordance with the Contract ;

THEREFORE, WE, ...........................(Name of the Bank) furnish you this Performance Guarantee in the manner hereinafter contained and agree with you as follows:

1. We, ..................................Bank do hereby undertake to pay the amounts due and payable under this Guarantee without any demur, merely on a demand, which has to be served on us before the expiry of this guarantee, time being essence of the contract, from you stating that the amount claimed is due by way of loss or damage caused to or would be caused to or suffered by you by reason of breach by the said vendor/ bidder of any of the terms and conditions contained in the Contract or by reason of the vendor/ bidder’s failure to perform the said contract. Any such demand made on us within the time stipulated above shall be conclusive as regards the amount due and payable by us under this guarantee. However, our liability under this guarantee shall be restricted to an amount not exceeding Rs.50% of work order (Rupees …………only).

2. We undertake to pay to you any money so demanded notwithstanding any dispute/s raised by the vendor/ bidder in any suit or proceeding before any Court or Tribunal relating thereto, our liability under these presents being absolute and unequivocal. The payment so made by us under this guarantee shall be a valid discharge of our liability for payment there under and the vendor/ bidder shall have no claim against us for making such payment.

We further agree that, if demand. as stated above, is made on us within the stipulated period, the guarantee herein contained shall remain in full force and effect and that it shall continue to be enforceable till all your dues under or by virtue of the said contract have been fully paid and your claims satisfied or discharged or till you certify that the terms and conditions of the said contract have been fully and properly carried out by the said vendor/ bidder and accordingly discharge this guarantee. Provided, however, serving of a written claim / demand in terms hereof on us for payment under this guarantee on or before the stipulated period , time being the essence of contract, shall be a condition precedent for accrual of our liability / your rights under this guarantee.

4. We further agree with you that you shall have the fullest liberty without our consent and without affecting in any manner our obligations hereunder, to vary any of the terms and conditions of the said Contract or to extend time for performance by the said vendor/ bidder from time to time or to postpone for any time or from time to time any of the powers exercisable by us against the said VENDOR/ BIDDER and to forbear or enforce any of the terms and conditions relating to the said Contract and we shall not be relieved from our liability by reason of such variation, or extension being granted to the said Vendor/ bidder or for any forbearance, act or omission on our part or any indulgence by us to the said vendor/ bidder or by any such matter or thing whatsoever which under the law relating to sureties would, but for this provision, have effect of so relieving us.

5. This Guarantee will not be discharged due to the change in the constitution of our SJCE-STEP or the Vendor/ bidder.

6. We lastly undertake not to revoke this guarantee during its currency except with your written consent.

NOTWITHSTANDING anything contained herein above;

i) Our liability under this Guarantee shall not exceed Rs.50% of the work order (Rupees …………only);

ii) This Guarantee shall be valid upto and including the warranty time period from the date of commissioning (mention date); and

iii) We are liable to pay the guaranteed amount or any part thereof under this Bank Guarantee only and only if you serve upon us a written claim or demand on or before the expiry of this guarantee.

Dated the ------------ day of --------2023

For and on behalf of

Branch Manager, Seal Address

**Annexure 9**

**COMMERCIAL’S OF THE OFFER FOR SERVER/WORKSTATION**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SI No.** | **Items** | **Item** | **Unit** | **Rate per item in Rs. Exclusive of taxes** | **Taxes in %** | **Total Price in Rs.** |
| 1 | 3D Scanner | Maker: Artec or Equivalent  Details: Hand Held Device  Technical specifications:   * Scanner type: handheld * 3D point accuracy,Up to 0.1 mm * 3D resolution,upto 0.5 mm   3D accuracy over distance, upto 0.1mm+0.3mm/m | 1 |  |  |  |
| 2 | CNC - Router | Maker: Stepcraft or Equivalent  Details: CNC Router (With MultiHeads & Ball Probe)  Technical specifications:   * Machine's Footprint (Width, Length, Height) : 36" x 48.3" x 25.4" * X-Travel : 679 mm * Y-Travel : 1044 mm   Z-Travel : 194 mm | 1 |  |  |  |
| 3 | 3D Printer - FDM | Maker: Divide by Zero or Equivalent  Details: Minimum Bed Size - 400\*300\*300  Technical specifications:   * Build Size: 400mm X 300mm X 300mm * NOZZLE Diameter: 0.4mm - 0.8mm ( optional ) * Extruder: Single ( upgradeable to dual ) * Noise Level: <55 dB   Accuracy 80-250 Micron | 1 |  |  |  |
| 4 | Laser Cutting Machine | Maker: VM Technologies Or Equivalent  Details : 4 Feet X 3 Feet  Technical specifications:   * Laser Type : CO2 * Working Area: 4 Feet X 3 Feet with all standard accessories | 1 |  |  |  |
| 5 | Laser Engraving Machine | Maker: [Yugma Impressions](https://www.copiainc.net/)  Details :  Technical specifications:   * Minimum line width: 0.01mm * Minimum character: 0.1mm * Marking speed: 0-7000m/s * Cooling system: air cooling * Repeat accuracy: 0.01mm * Input power: AC 220V 10% 50Hz (60Hz) * Lifetime: 100,000 hours (if properly operated) * Maintenance Free Laser Engine * Motorized or Manual Z-Adjustment * Easily Integrated Footprint | 1 |  |  |  |
| 6 | 3D Printer - SLA | Maker: [Prusa or Equivalent](https://www.copiainc.net/)  Technical specifications:   * LCD resolution 5.96'', 2560×1620p * LCD lifespan / warranty 2000 hours * Minimum Print volume size 127×80×150 mm * Layer exposure time 1.3 - 2.4 seconds depending on material and layer height * Tilt time 3 seconds   with all standard accessories | 1 |  |  |  |
| 7 | CNC wire EDM Cutting Machine | Maker: Fostex Or Equivalent  Technical specifications:   * CNC-wire cut Electric discharge machine with single cut Control Cabinet (3 Phase, 45V/50Hz) * and standard accessories steel cover, LM Guide, High Pressure coolant pump & tool Box. | 1 |  |  |  |

Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (name)

on behalf of

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Name of the vendor/ bidder)

Note:

1. The vendor/ bidder are required to fill the columns with the price Schedule in numeric INR only (No NA/blank column/ - / NIL etc.)
2. The above rates are for units. However, at the time of the Work order & settling of bills, the actual consumption will be taken into account.

**Annexure – 10**

**Experience Details (Customer References)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Sl.No. | Name of the Organization | Contact Person | Contact Telephone no, email id and Address | Date/ Period of Implementation | No. of printers and related accessories installed | Type of supporting document submitted |
| 1 |  |  |  |  |  |  |
| 2 |  |  |  |  |  |  |
| 3 |  |  |  |  |  |  |
| 4 |  |  |  |  |  |  |
| 5 |  |  |  |  |  |  |

Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (name)

on behalf of

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Name of the vendor/ bidder)

Note: Please fill this form and submit the supporting documents for each customer reference. Failing the same may lead to the rejection of the bid. You may add the customer references by adding multiple rows.

EMDs for the Individual equipment are as below.

|  |  |  |
| --- | --- | --- |
| **SI No.** | **Items** | **EMD** |
| 1 | 3D Scanner | Rs. 25,000.00/- |
| 2 | CNC - Router | Rs. 31,250.00/- |
| 3 | 3D Printer - FDM | Rs. 18,750.00/- |
| 4 | Laser Cutting Machine | Rs. 16,250.00/- |
| 5 | Laser Engraving Machine | Rs. 10,000.00/- |
| 6 | 3D Printer - SLA | Rs. 8,125.00/- |
| 7 | CNC wire EDM Cutting Machine | Rs. 12,500.00/- |